**中天伊丽洁100公斤全自动洗脱机季促销进行中**

**中天伊丽洁全自动洗脱机产品介绍：采用全电脑液晶人机对话操作界面，中文显示超大屏幕，有30种不同的洗涤程序可供选择，可满足任何洗涤要求，全面实现洗、漂、汰等过程的自动化。中天伊丽洁全自动工业洗衣机采用悬浮式避振结构，配以弹簧阻尼系统，超低振动，可安全放置在任何楼层，无需做地基。先进的变频调速系统，调速方便，低电流启动，省电节能效果明显，运行平稳噪音低，传动结构简单可靠。 全封闭后排水框架结构设计，减少污染，保持工作场地干燥清洁。内外筒均为不锈钢。提高了使用寿命。 不锈钢精制门，气动安全装置，极大提高了使用中的安全性。后置浓油润滑泵设计，实现传动系统润滑剂自动加油，更先进，更人性化的关怀。**

Elige 50-100kg automatic washing machine promotion in the season Elige automatic washing machine product introduction: using the all-computer LCD man-machine dialogue operation interface, Chinese display super-large screen, there are 30 different washing procedures to choose from, can meet any washing requirements, the full realization of washing, bleaching, elimination process automation. It adopts suspension structure and spring damping system, so it can be safely placed on any floor without foundation. Using frequency conversion speed control system, speed convenient, low current start, energy saving effect is obvious, running stable low noise, transmission structure simple and reliable. Fully enclosed drainage frame structure design, reduce pollution, keep the workplace dry and clean. Both inner and outer cylinders are stainless steel. The utility model improves the service life of the utility model. Stainless steel refined door, pneumatic safety device, greatly improve the safety in use. After the thick oil lubrication pump design, to achieve transmission system lubricant automatic oiling, more advanced, more humane care.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| model |  XGQ-15F |  XGQ-20F |  XGQ-25F |  XGQ-30F |
| Washing capacity(kg) |  15 |  20 |  25 |  30 |
| Size of inner barrel(Diameter \* depth)mm |  700\*400 |  700\*540 |  800\*500 |  800\*590 |
| Wash rpm |  50 |  50 |  48 |  48 |
| High spin speed(rpm) |  860 |  860 |  800 |  800 |
|  Power Supply( V/P/HZ) |  (220V/)380V/3/50HZ |  ( 220V/)380V/3/50HZ |   (220V/)380V/3/50HZ |  380V/3/50HZ |
| Electric heating power(kw) |  6 |              6/9 |  6/9 |  12 |
| Motor rated power (KW) |  1.5 |  2.2 |  2.2 |  3 |
|  External dimensions(Wide \* deep \* high) |  1100\*1050\*1500 | 1100\*1160\*1500 |  1200\*1120\*1600 |  1320\*1280\*1800 |
|  Weight of the whole machine(kg) |  550 | 650 |  750 |  1000 |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| model |  XGQ-15F |  XGQ-20F |  XGQ-25F |  XGQ-30F |
| model |  XGQ-50F |  XGQ-100F |  XGQ-120F |  XGQ-150F |
| Washing capacity(kg) |  50 | 100 |  120 |  150 |
| Size of inner barrel(Diameter \* depth)mm | 1080\*600 | 1200\*850 |  1300\*885 |  1400\*1000 |
| Wash rpm | 44 | 35 | 33 | 28 |
| High spin speed(rpm) | 720 |  650 | 630 |  600 |
|  Power Supply( V/P/HZ) | 380V/3/50HZ | 380V/3/50HZ |   380V/3/50HZ | 380V/3/50HZ |
| Electric heating power(kw) | 18 |        24     | 36  | /  |
| Motor rated power (KW) | 4 | 7.5 |  11 |  12 |
|  External dimensions(Wide \* deep \* high) | 1530\*1760\*1780 | 1760\*1900\*2100 |  1765\*1910\*1950 |  1900\*2200\*2150 |
|  Weight of the whole machine(kg) | 1600 | 2600 |  3000 | 3600 |